Judd-modified CIE 2-deg colour matching functions (1951)

Data key

Columns

1. Wavelength (nm) 

2. 
[image: image1.wmf]()

x

l


3. 
[image: image2.wmf]()

y

l

 

4. 
[image: image3.wmf]()

z

l

 



Notes

It has long been clear that the CIE 1924 V(l) function (CIE, 1926) that was used to construct the CIE 1931 2-deg CMFs (CIE, 1931) seriously underestimates sensitivity at wavelengths below 460 nm. Judd (1951) proposed a revised version of V() to overcome this problem, and derived a new set of CMFs. Yet, like the CIE 1931 CMFs, the Judd-modified functions are reconstructed using the V() function. 

From Table 1(5.5.2) of Wyszecki and Stiles (1982). 
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