Judd-Vos-modified CIE 2-deg colour matching functions (1978)
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Notes

    In 1978, Vos made additional corrections to Judd's (1951) revision of the CIE 1931 2 deg color matching functions (CIE, 1932) and incorporated the infra-red color reversal described by Brindley (1955). The Judd-Vos V(l) is the modified luminosity function VM(l) recently adopted by the CIE. 

From Table 1 of Vos(1978). See also Table I(5.5.2) of Wyszecki and Stiles (1982). 
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